c)

Ripple on the magnetizing branch current is 3.5 A. Therefore, at the boundary of CCM and DCM, average inductor current is 1.75 A. Input power is

Output power is 8.4W if the losses are neglected. Output current is