Q2)

For controlling the output voltage, we need to design a controller which feedback the output voltage to the gate driver of the switch which determines the duty cycle. In design procedure, we should pay attention to keep a stabilized operation of the converter. For this purpose, gain of the error amplifier at switching frequency should be low. Moreover, we should keep phase margin of the controller at least -45 degree.